	▣ 원화홀 장비 목록
콘솔 Console		제조사 Manufacturer / 모델 Model		입력 Input	출력 Output	수량 Quantity	비고 Remarks
		YAMAHA / PM5D		48ch	24ch	1
형 식 Type			제조사 Manufacturer / 모델 Model			수량 Quantity	비고 Remarks
SPEAKER		MAIN SPEAKER	Meyer Sound / UPQ-1P			2	POWERED SPEAKER
		CENTER SPEAKER	Meyer Sound / UPJ-1P			2	POWERED SPEAKER
		SUB WOOFER SPEAKER	Meyer Sound / 500-HP			2	POWERED SPEAKER
		SIDE FILL SPEAKER 1	Meyer Sound / UPA-1P			2	POWERED SPEAKER
		SIDE FILL SPEAKER 2	Meyer Sound / UPJ-1P			2	POWERED SPEAKER
		STAGE MONITOR SPEAKER	Meyer Sound / UM-100P			6	POWERED SPEAKER
PLAYER / RECORDER		COMPACT DISK PLAYER	Numark / CDN88MP3			1
		COMPACT DISK RECORDER	Tascam / CD RW-901 SL			1
		MINI DISK RECORDER	Tascam / MD-350			2
		CASSETTE DECK	Tascam / 202MKIV			1
Effects / Processor		SIGNAL PROCESSOR	Meyer Sound / GALILEO408			1
		EQUALIZE	LA Audio / EQ231G-SP			2

경주예술의전당 원화홀 장비 목록

형 식 Type		제조사 Manufacturer / 모델 Model	수량 Quantity	비고 Remarks
MICROPHONE	WIRELESS MICROPHONE	Shure / ULXP 4	5	900 MHz 5ea
		Shure / ULX 2 / BETA 87A	5	900 MHz 5ea
		Shure / ULX 1	5	900 MHz 5ea
	▪ 단, 900MHz는 로드안테나입니다.

음향 전용 전력 Electric Power	3상4선 30KW 37.5KVA		F O H
	3상4선 26KW 32.5KVA		무대
	UPS – 5 KVA		F O H